**ESS-DIVE Metadata for Thresholds Data Package**

**Title**:

Data and scripts associated with “Thresholds of Area Burned and Burn Severity for Downstream Riverine Systems to ‘Feel the Burn’”

**Alternative Identifiers:**

**Abstract:**

This data package is associated with the publication “Thresholds of Area Burned and Burn Severity for Downstream Riverine Systems to ‘Feel the Burn’” submitted to Water Resources Research (Wampler et al. 2025).

This study used the Soil and Water Assessment Tool (SWAT), a processed based model to explore the impacts of area burned and burn severity on streamflow, nitrate, and dissolved organic carbon (DOC) in two test basins: a semi-arid, mixed land use basin and a humid, primarily forested basin. We developed 1800 wildfire scenarios that we ran in each basin: 20 different burn extents (5 to 100% by 5%), 3 different burn severities (low, moderate, and high), and 30 different post-fire precipitation scenarios. We also ran an additional 30 scenarios associated with no wildfire for the 30 post-fire precipitation scenarios. For each scenario we were interested in the change in runoff ratio (streamflow) and average concentration and annual loads (nitrate and DOC) across the wildfire scenarios.

This data package contains the data and scripts required to build SWAT models for the two test basins, create and run the wildfire scenarios, and generate the data summaries and figures used in the associated manuscript.

This dataset contains (1) file-level metadata; (2) data dictionary; (3) data package readme; (4) workflow documentation; (5) a folder with model input data (“inputs”); (6) a folder with model output data (“outputs”); and (7) a folder with scripts needed to create and run the models and analyze the outputs (“scripts”). The input data folder contains the following items: (1) a DOC/wildfire module where the DOC outputs are in kilograms per time step (Wampler et al. 2023); (2) a DOC/wildfire module where the DOC outputs are in milligrams per liter; (3) a modified SWAT-CUP (<https://www.2w2e.com/home/SwatCup>) file with absolute parameter values; (4) a .csv file with calibrated parameter values for both models; (5) a .txt file called “model.in” with updated parameters for the DOC module; and (6) a .pdf with directions for using the wildfire module. The folder with model output data contains three subfolders: (1) “data”, which contains the processed model outputs; (2) “figures”, which contains the figures from the manuscript; and (3) “summary-outputs”, which contains summarized data used to create tables and results for the manuscript. This package contains the following file types: csv, exe, in, txt, pdf, R, png.

**Keywords**:

Wildfire

Streams

Dissolved organic matter

Biogeochemistry

River corridor

ESS-DIVE CSV File Formatting Guidelines Reporting Format

ESS-DIVE File Level Metadata Reporting Format

ESS-DIVE Hydrologic Monitoring Reporting Format

ESS-DIVE Model Data Archiving Guidelines

**Data variables:**

Precipitation

Evapotranspiration

Nitrate

Dissolved Organic Carbon

Streamflow

**Pub date**:

**Data usage rights**:

Creative Commons Attribution

**Project**:

River Corridor and Watershed Biogeochemistry SFA

**Funding org:**

U.S. DOE > Office of Science > Biological and Environmental Research (BER)

**DOE Contracts**:

DOE Award #54737

**Related reference**:

Wampler, K. A., Myers-Pigg, A. N., Kang, H., Regier, P., Scheibe, T. D., and Bladon, K. D. (2025). Thresholds of Area Burned and Burn Severity for Downstream Riverine Systems to ‘Feel the Burn’. ESS Open Archive [preprint].

Boye, K., Crystal-Ornelas, R., O'Ryan, D., Goldman, A. E., Damerow, J., Varadharajan, C., & Agarwal, D. (2022). ESS-DIVE Reporting Format for Sample-based Water and Soil Chemistry Measurements. Environmental Systems Science Data Infrastructure for a Virtual Ecosystem (ESS-DIVE), ESS-DIVE repository. doi: 10.15485/1865731

Wampler, K. A., Bladon, K. D., & Faramarzi, M. (2023). Modeling wildfire effects on streamflow in the Cascade Mountains, Oregon, USA. Journal of Hydrology, 621, 129585. <https://doi.org/10.1016/j.jhydrol.2023.129585>

2W2E GmbH. (2019). SWAT-CUP. Zürich, Switzerland: Water Weather Energy Ecosystem. Available from [https://www.2w2e.com/home/SwatCup](https://www.2w2e.com/home/SwatCup%20)

Agarwal, D., Cholia, S., Hendrix, V. C., Crystal-Ornelas, R., Snavely, C., Damerow, J., & Varadharajan. (2022). ESS-DIVE Reporting Format for Dataset Metadata. Environmental Systems Science Data Infrastructure for a Virtual Ecosystem (ESS-DIVE), ESS-DIVE repository. https://doi.org/10.15485/1866026

Velliquette, T., Welch, J., Crow, M., Devarakonda, R., Heinz, S., Crystal-Ornelas, R. (2021). ESS-DIVE Reporting Format for Comma-separated Values (CSV) File Structure. Environmental Systems Science Data Infrastructure for a Virtual Ecosystem (ESS-DIVE), ESS-DIVE Repository. <https://doi.org/10.15485/1734841>

Velliquette, T., Welch, J., Crow, M., Devarakonda, R., Heinz, S., Crystal-Ornelas, R. (2021). ESS-DIVE Reporting Format for File-level Metadata. Environmental Systems Science Data Infrastructure for a Virtual Ecosystem (ESS-DIVE), ESS-DIVE Repository. https://doi.org/10.15485/1734840

**Principal investigator:**

Scheibe

**Contact name**:

Katie Wampler

**Contact email**:

Katie.wampler@oregonstate.edu

**Creators**:

Katie Wampler

Kevin Bladon

Brieanne Forbes

Hyunwoo Kang

Beck Powers-McCormack

Peter Regier

Tim Scheibe

Allison Myers-Pigg

**Start date**:

2017-08-11

**End date**:

2018-08-10

**Location description**:

The semi-arid basin was based on data from the Tule River Basin in California, USA (USGS gage 11204100).

The humid basin was based on data from the American River Basin in Washington, USA (USGS gage 12488500)

**Coordinates**:

American: 46.97761606 , -121.168696

Tule: 36.02411648, -118.8134258

**Methods:**

This data package includes R scripts (“scripts”) which are numbered in ascending order of use to reproduce the model and results from the associated manuscript. While most of the data is pulled via R from publicly available data sources, a few additional files are needed to create the models which are located in the “inputs” folder. This folder also contains two different versions of the SWAT wildfire module. For specific details on workflow steps see “thresholds\_workflow.pdf”. Model outputs can be found in the “outputs/data” folder, while figures and summary tables used in the manuscript are in “outputs/figures” and “outputs/summary-outputs” respectively.